**References**

Armillotta, A., Bellotti, M., & Cavallaro, M. (2018). Warpage of FDM parts: Experimental tests and analytical model. *Robotics and Computer-Integrated Manufacturing*, *50,* 140-152. doi: 10.1016/j.rcim.2017.09.007

Baich, L., Manogharan, G., & Marie, H. (2015). Study of infill print design on production cost-time of 3D printed ABS parts. *International Journal of Rapid Manufacturing, 5*, 308-311. doi:10.1504/ijrapidm.2015.074809

Deng, C., Kang, J., Shangguan, H., Hu, Y., Huang, T., & Liu, Z. (2018). Effects of hollow structures in sand mold manufactured using 3D printing technology. *Journal of Materials Processing Technology*, 255, 516-523. doi:10.1016/j.jmatprotec.2017.12.031

Dizon, J. R. C., Espera, A. H., Chen, Q., & Advincula, R. C. (2018). Mechanical characterization of 3D-printed polymers. *Additive Manufacturing, 20*, 44-67. doi:10.1016/j.addma.2017.12.002

Flaata, T., Michna, G. J., & Letcher, T. (2017). Thermal conductivity testing apparatus for 3D printed materials. *Proceedings of the ASME Summer Heat Transfer Conference*. doi:10.1115/HT2017-4856

Haertel, J. H. K., & Nellis, G. F. (2017). A fully developed flow thermofluid model for topology optimization of 3D-printed air-cooled heat exchanger. *Applied Thermal Engineering*, *119*, 10-24. doi:10.1016/j.applthermaleng.2017.03.030

Han, Y. (2016). Influence of 3D printing infill patterns on the effective thermal properties. *Journal of Purdue Undergraduate Research*, 6(89). doi:10.5703/1288284316207

Kim, D. M., & Viskanta, R. (1984). Heat transfer by conduction, natural convection and radiation across a rectangular cellular structure. *International Journal of Heat and Fluid Flow, 5*, 205-213. doi:10.1016/0142-727X(84)90053-5

Larkin, B. K., & Churchill, S. W. (1959). Heat transfer by radiation through porous insulations. *AIChE Journal*, 5, 467-474. doi:10.1002/aic.690050413

Mathur, D. S. (1970). *Fundamentals of Heat*. Amir Chand Marg (Nai Sarak), Delhi-6: Sultan Chand and Sons.

Mehrizi, A. A., Farhadi, M., Sedighi, K., & Delevar, A. (2013). Effect of fin position and porosity on heat transfer improvement in a plate porous media heat exchanger. *Journal of the Taiwan Institute of Chemical Engineers, 44*, 420-431. doi:10.1016/j.jtice.2012.12.018

Trhlíková, L., Zmeskal, O., Psencik, P., & Florian, P. (2016). Study of the thermal properties of filaments for 3D printing. *AIP Conference Proceedings, 1752*. doi:10.1063/1.4955258

Ultimaker. (2018). *How to fix warping.* Retrieved from ultimaker.com/en/resources/19537-how-to-fix-warping.

Wang, Y., Yan, J., Zhang, X., Pan, Y. (2015). Effect of surface thermal radiation on natural convection and heat transfer in a cavity containing a horizontal porous layer. *Procedia Engineering, 121*, 1193-1199. doi:10.1016/j.proeng.2015.09.137

Zhang, J., Wang, X. Z., Yu, W. W., Deng, Y. H. (2017). Numerical investigation of the influence of process conditions on the temperature variation in fused deposition modeling. Materials & Design, 130, 59-68. doi:10.1016/j.matdes.2017.05.040

Zhuang, Y., Song, W., Ning, G., Sun, X., Sun, Z., Xu, G., … Tao, S. (2017). 3-D printing of materials with anisotropic heat distribution using conductive polylactic acid composites. *Materials & Design*, *126*, 135-140. doi:10.1016/j.matdes.2017.04.047